Exercise7-3

I think RAID 6 is the best choice. In the case of RAID 0, the access speed is fast, but I think the safety priority of important data is the most important. With RAID 6, data is saved up to two simultaneous failures.